# RuleeSmart – User Guide

Victor Climate - Board V1

1. 相关资源
   1. VOC传感器SGP-30
   2. 温湿度传感器AHT-10
   3. 程序代码 <https://github.com/ruleechen/home-climate>
2. 已知问题
   1. 目前温湿度传感器太靠近主控芯片，受到主控芯片发热的影响，温湿度指标偏差比较大。
   2. 鉴于温湿度有偏差，温湿度指标作为辅助空气质量检测的指标，会部分影响到空气质量指标。

A picture containing text, electronics, circuit

Description automatically generated

## 初次上电后会看到指示灯闪烁，提示没有wifi连接。用手机或电脑靠近设备并查找设备的接入点，接入点名字为VIC-开头，后面接着6位设备ID。

A screenshot of a phone

Description automatically generated with medium confidence

1. 连接上设备的接入点之后，用浏览器打开<http://192.168.4.1>进入设备的管理配置后台。如果遇到打不开的情况，要稍等一下多刷新几次。进入管理界面后依次点击WiFi --> Join --> 选择WiFi --> 输入密码 --> Join按钮，加入家里的网络。
   1. 连接上家里的网络后，如果需要进行更多的配置，可以用浏览器在同一个WiFi网络下打开<http://vic-a2a051.local>进入管理界面。

Graphical user interface, text, application

Description automatically generated

1. 等待设备连接上WiFi，连接上之后指示灯停止闪烁。用苹果设备自带的Home app开始添加设备。设备的验证密码为8个1，添加过程会用到。
   1. 如果设备添加失败，可以长按设备上的按钮10秒以上，放开按钮后会重置配对信息，重新开始配置过程。

Graphical user interface, application

Description automatically generated

Text

Description automatically generated

Graphical user interface, text, application, chat or text message

Description automatically generated

Text

Description automatically generated

Graphical user interface, text, application, chat or text message

Description automatically generated

Graphical user interface

Description automatically generated with medium confidence

A screenshot of a cell phone

Description automatically generated with medium confidence

A screenshot of a phone

Description automatically generated with medium confidence